Processing node 32 link 1 session 6

-------------------------------------------------------------------
[                F A M I L Y    G R O U P I N G                   ]
-------------------------------------------------------------------
A GND block GND U11 if part of family 1
A component GND U11 if part of family 1
{ surfing node 32 }
A component EOUTPUT OUT5 if part of family 1
  { exploring component EOUTPUT OUT5 }
  { surfing node 34 }
A component EINPUT IN5 if part of family 1
    { exploring component EINPUT IN5 }
    { surfing node 33 }
A component PWR U10 if part of family 1
      { exploring component PWR U10 }
    { exiting due source component PWR U10 }
  { exiting node 34 }
{ exiting node 32 }

-------------------------------------------------------------------------------------------------
[    P H A S E    1    -    E x p l o r i n g    T R E E    ,    a d d    S U M    n o d e s    ]
-------------------------------------------------------------------------------------------------
{ Exploring node 32 which consist of 2 links }
  Plug <B> of Comp <EOUTPUT> REF=<OUT5> Node <32> assigned as OUTPUT
  Plug <A> of Comp <EOUTPUT> REF=<OUT5> Node <34> assigned as INPUT
  (|) Slowly opening door of link 0 in node 32
  (i) Component EOUTPUT OUT5 is part of the population for node 32
  Surfing inputs for component <EOUTPUT> <OUT5>
  (i) Component EOUTPUT OUT5 has 2 pins
  Invoking ExploreTree for Node 34 coming from the bidirectional a PLUG <A> of COMPONENT <EOUTPUT> REF=<OUT5>
  { Exploring node 34 which consist of 2 links }
    Plug <B> of Comp <EINPUT> REF=<IN5> Node <34> assigned as OUTPUT
    Plug <A> of Comp <EINPUT> REF=<IN5> Node <33> assigned as INPUT
    (|) Slowly opening door of link 0 in node 34
    (i) Link 0 of node 34 skipped because it is the enter node
    (|) Slowly opening door of link 1 in node 34
    (i) Component EINPUT IN5 is part of the population for node 34
    Surfing inputs for component <EINPUT> <IN5>
    (i) Component EINPUT IN5 has 2 pins
    Invoking ExploreTree for Node 33 coming from the bidirectional a PLUG <A> of COMPONENT <EINPUT> REF=<IN5>
    { Exploring node 33 which consist of 2 links }
      (|) Slowly opening door of link 0 in node 33
      (i) Component PWR U10 is part of the population for node 33
      Surfing inputs for component <PWR> <U10>
      (i) Component PWR U10 has 1 pins
      { End exploring node 33 - Tree is POWERED(+) }
      ($) Link 0 of node 33 linked to plug VCC of PWR U10 DOES produce power
    (R) After evaluating node <33> these are the results:
      -> 1 components result to be the population of the forest
      -> 1 links are SOURCED
    { End exploring node 33 - Tree is POWERED(+) }
    Plug B of EINPUT IN5 produces source for the node 34
    (x) Link 0 of node 34 linked to plug A of EOUTPUT OUT5 is an input and requires power
    ($) Link 1 of node 34 linked to plug B of EINPUT IN5 DOES produce power
  (R) After evaluating node <34> these are the results:
    -> 1 components result to be the population of the forest
    -> 1 link is THE ENTER NODE
    -> 2 links are SOURCED
    -> 1 times a node is marked as one-to-one
  { End exploring node 34 }
  Plug B of EOUTPUT OUT5 produces source for the node 32
  (|) Slowly opening door of link 1 in node 32
  (i) Link 1 of node 32 skipped because it is the enter node
  ($) Link 0 of node 32 linked to plug B of EOUTPUT OUT5 DOES produce power
  (x) Link 1 of node 32 linked to plug OUT of GND U11 is an input and requires power
(R) After evaluating node <32> these are the results:
  -> 1 components result to be the population of the forest
  -> 1 link is THE ENTER NODE
  -> 2 links are SOURCED
  -> 1 times a node is marked as one-to-one
{ End exploring node 32 }

------------------------------------------------------------------------------------------
[    P H A S E    2    -    P l a c i n g    R E A D    /    W R I T E    B l o c k s    ]
------------------------------------------------------------------------------------------

------------------------------------------------------------------------
[    P H A S E    3    -    P l a c i n g    C A S T    B L O C K S    ]
------------------------------------------------------------------------

| Terminal component found by session 6 , GND U11 attached to [32/1] |


[---> STARTING TREE [32/1] GND U11 <---] 


-------------------------------------------------------------------
[    P H A S E    4    -    G e n e r a t i n g    P - C o d e    ]
-------------------------------------------------------------------
(STARTING FUNCTION BLOCK <EOUTPUT> REF=<OUT5>)
  (STARTING FUNCTION BLOCK <EINPUT> REF=<IN5>)
    (+) <PWR> POWER COMPONENT REF=<U10>
    (C) PLACING <EINPUT> COMPONENT REF=<IN5>
  (ENDING FUNCTION BLOCK <EINPUT> REF=<IN5>)

  (C) PLACING <EOUTPUT> COMPONENT REF=<OUT5>
(ENDING FUNCTION BLOCK <EOUTPUT> REF=<OUT5>)

Depolarizing EOUTPUT OUT5
Depolarizing EINPUT IN5
