
------------------------------------------------------------------------------
Symbol meaning:

(+) = Power component
(-) = GND component
(Z) = Zero component
(M) = Member calling
(S) = Store value
(C) = Component main function placing (ActionFx or walk through)
(W) = Network break write
(R) = Network break read
------------------------------------------------------------------------------


-------------------------------------------------------------------
[    G N D    T O    Z E R O    S U B S T I T U T I O N           ]
-------------------------------------------------------------------

-------------------------------------------------------------------
[           S I N G L E    P O W E R    F E E D I N G            ]
-------------------------------------------------------------------

-------------------------------------------------------------------
[           S I N G L E    G R O U N D    F E E D I N G           ]
-------------------------------------------------------------------

----- Start Recurse -----

| terminal component found by coord (736,72), GND U7 attached to [22/1] |


| terminal component found by coord (344,80), GND U1 attached to [10/0] |


| terminal component found by coord (344,128), GND U5 attached to [20/0] |


| terminal component found by coord (344,176), GND U4 attached to [6/1] |


| terminal component found by coord (344,224), GND U8 attached to [30/0] |


| terminal component found by coord (344,272), GND U11 attached to [32/1] |


| terminal component found by coord (736,72), GND U7 attached to [22/1] |

+---------------------------------------------------------------------------+
|                                                                           |
| S E S S I O N       1                                                     |
|                                                                           |
+---------------------------------------------------------------------------+
Processing node 22 link 1 session 1

-------------------------------------------------------------------
[                F A M I L Y    G R O U P I N G                   ]
-------------------------------------------------------------------
A GND block GND U7 if part of family 1
A component GND U7 if part of family 1
{ surfing node 22 }
A component OUTPUT OUT16 if part of family 1
  { exploring component OUTPUT OUT16 }
  { surfing node 24 }
A component CLOCK CLK1 if part of family 1
    { exploring component CLOCK CLK1 }
  { exiting node 24 }
{ exiting node 22 }

-------------------------------------------------------------------------------------------------
[    P H A S E    1    -    E x p l o r i n g    T R E E    ,    a d d    S U M    n o d e s    ]
-------------------------------------------------------------------------------------------------
{ Exploring node 22 which consist of 2 links }
  Plug <B> of Comp <OUTPUT> REF=<OUT16> Node <22> assigned as OUTPUT
  Plug <A> of Comp <OUTPUT> REF=<OUT16> Node <24> assigned as INPUT
  (|) Slowly opening door of link 0 in node 22
  (i) Component OUTPUT OUT16 is part of the population for node 22
  Surfing inputs for component <OUTPUT> <OUT16>
  (i) Component OUTPUT OUT16 has 2 pins
  Invoking ExploreTree for Node 24 coming from the bidirectional a PLUG <A> of COMPONENT <OUTPUT> REF=<OUT16>
  { Exploring node 24 which consist of 2 links }
    (|) Slowly opening door of link 0 in node 24
    (i) Link 0 of node 24 skipped because it is the enter node
    (|) Slowly opening door of link 1 in node 24
    (i) Component CLOCK CLK1 is part of the population for node 24
    Surfing inputs for component <CLOCK> <CLK1>
    (i) State component CLOCK CLK1 was marked as evaluated
    (i) Component CLOCK CLK1 has 1 pins
    (+S+) Assuming link is powered by OUT which is the single output of a state component COMPONENT=<CLOCK> REF=<CLK1>
    (x) Link 0 of node 24 linked to plug A of OUTPUT OUT16 is an input and requires power
    ($) Link 1 of node 24 linked to plug OUT of CLOCK CLK1 DOES produce power
  (R) After evaluating node <24> these are the results:
    -> 1 components result to be the population of the forest
    -> 1 link is THE ENTER NODE
    -> 2 links are SOURCED
    -> 1 links contains STATE ELEMENTS
    -> 1 times a node is marked as one-to-one
  { End exploring node 24 }
  Plug B of OUTPUT OUT16 produces source for the node 22
  (|) Slowly opening door of link 1 in node 22
  (i) Link 1 of node 22 skipped because it is the enter node
  ($) Link 0 of node 22 linked to plug B of OUTPUT OUT16 DOES produce power
  (x) Link 1 of node 22 linked to plug OUT of GND U7 is an input and requires power
(R) After evaluating node <22> these are the results:
  -> 1 components result to be the population of the forest
  -> 1 link is THE ENTER NODE
  -> 2 links are SOURCED
  -> 1 times a node is marked as one-to-one
{ End exploring node 22 }

------------------------------------------------------------------------------------------
[    P H A S E    2    -    P l a c i n g    R E A D    /    W R I T E    B l o c k s    ]
------------------------------------------------------------------------------------------

------------------------------------------------------------------------
[    P H A S E    3    -    P l a c i n g    C A S T    B L O C K S    ]
------------------------------------------------------------------------

| Terminal component found by session 1 , GND U7 attached to [22/0] |


[---> STARTING TREE [22/1] GND U7 <---] 


-------------------------------------------------------------------
[    P H A S E    4    -    G e n e r a t i n g    P - C o d e    ]
-------------------------------------------------------------------
(STARTING FUNCTION BLOCK <OUTPUT> REF=<OUT16>)
  (STARTING FUNCTION BLOCK <CLOCK> REF=<CLK1>)
    (C) PLACING <CLOCK> COMPONENT REF=<CLK1>
  (ENDING FUNCTION BLOCK <CLOCK> REF=<CLK1>)

  (M) <CLOCK/OUT> MEMBER CALLING REF=<CLK1>
  (C) PLACING <OUTPUT> COMPONENT REF=<OUT16>
(ENDING FUNCTION BLOCK <OUTPUT> REF=<OUT16>)

Depolarizing OUTPUT OUT16

| terminal component found by coord (344,80), GND U1 attached to [10/0] |

+---------------------------------------------------------------------------+
|                                                                           |
| S E S S I O N       2                                                     |
|                                                                           |
+---------------------------------------------------------------------------+
Processing node 10 link 0 session 2

-------------------------------------------------------------------
[                F A M I L Y    G R O U P I N G                   ]
-------------------------------------------------------------------
A GND block GND U1 if part of family 1
A component GND U1 if part of family 1
{ surfing node 10 }
A component EOUTPUT OUT1 if part of family 1
  { exploring component EOUTPUT OUT1 }
  { surfing node 3 }
A component EINPUT IN1 if part of family 1
    { exploring component EINPUT IN1 }
    { surfing node 8 }
A component PWR U2 if part of family 1
      { exploring component PWR U2 }
    { exiting due source component PWR U2 }
  { exiting node 3 }
{ exiting node 10 }

-------------------------------------------------------------------------------------------------
[    P H A S E    1    -    E x p l o r i n g    T R E E    ,    a d d    S U M    n o d e s    ]
-------------------------------------------------------------------------------------------------
{ Exploring node 10 which consist of 2 links }
  Plug <B> of Comp <EOUTPUT> REF=<OUT1> Node <10> assigned as OUTPUT
  Plug <A> of Comp <EOUTPUT> REF=<OUT1> Node <3> assigned as INPUT
  (|) Slowly opening door of link 0 in node 10
  (i) Link 0 of node 10 skipped because it is the enter node
  (|) Slowly opening door of link 1 in node 10
  (i) Component EOUTPUT OUT1 is part of the population for node 10
  Surfing inputs for component <EOUTPUT> <OUT1>
  (i) Component EOUTPUT OUT1 has 2 pins
  Invoking ExploreTree for Node 3 coming from the bidirectional a PLUG <A> of COMPONENT <EOUTPUT> REF=<OUT1>
  { Exploring node 3 which consist of 2 links }
    Plug <B> of Comp <EINPUT> REF=<IN1> Node <3> assigned as OUTPUT
    Plug <A> of Comp <EINPUT> REF=<IN1> Node <8> assigned as INPUT
    (|) Slowly opening door of link 0 in node 3
    (i) Component EINPUT IN1 is part of the population for node 3
    Surfing inputs for component <EINPUT> <IN1>
    (i) Component EINPUT IN1 has 2 pins
    Invoking ExploreTree for Node 8 coming from the bidirectional a PLUG <A> of COMPONENT <EINPUT> REF=<IN1>
    { Exploring node 8 which consist of 2 links }
      (|) Slowly opening door of link 0 in node 8
      (i) Link 0 of node 8 skipped because it is the enter node
      (|) Slowly opening door of link 1 in node 8
      (i) Component PWR U2 is part of the population for node 8
      Surfing inputs for component <PWR> <U2>
      (i) Component PWR U2 has 1 pins
      { End exploring node 8 - Tree is POWERED(+) }
      ($) Link 1 of node 8 linked to plug VCC of PWR U2 DOES produce power
    (R) After evaluating node <8> these are the results:
      -> 1 components result to be the population of the forest
      -> 1 link is THE ENTER NODE
      -> 1 links are SOURCED
    { End exploring node 8 - Tree is POWERED(+) }
    Plug B of EINPUT IN1 produces source for the node 3
    (|) Slowly opening door of link 1 in node 3
    (i) Link 1 of node 3 skipped because it is the enter node
    ($) Link 0 of node 3 linked to plug B of EINPUT IN1 DOES produce power
    (x) Link 1 of node 3 linked to plug A of EOUTPUT OUT1 is an input and requires power
  (R) After evaluating node <3> these are the results:
    -> 1 components result to be the population of the forest
    -> 1 link is THE ENTER NODE
    -> 2 links are SOURCED
    -> 1 times a node is marked as one-to-one
  { End exploring node 3 }
  Plug B of EOUTPUT OUT1 produces source for the node 10
  (x) Link 0 of node 10 linked to plug OUT of GND U1 is an input and requires power
  ($) Link 1 of node 10 linked to plug B of EOUTPUT OUT1 DOES produce power
(R) After evaluating node <10> these are the results:
  -> 1 components result to be the population of the forest
  -> 1 link is THE ENTER NODE
  -> 2 links are SOURCED
  -> 1 times a node is marked as one-to-one
{ End exploring node 10 }

------------------------------------------------------------------------------------------
[    P H A S E    2    -    P l a c i n g    R E A D    /    W R I T E    B l o c k s    ]
------------------------------------------------------------------------------------------

------------------------------------------------------------------------
[    P H A S E    3    -    P l a c i n g    C A S T    B L O C K S    ]
------------------------------------------------------------------------

| Terminal component found by session 2 , GND U1 attached to [10/1] |


[---> STARTING TREE [10/0] GND U1 <---] 


-------------------------------------------------------------------
[    P H A S E    4    -    G e n e r a t i n g    P - C o d e    ]
-------------------------------------------------------------------
(STARTING FUNCTION BLOCK <EOUTPUT> REF=<OUT1>)
  (STARTING FUNCTION BLOCK <EINPUT> REF=<IN1>)
    (+) <PWR> POWER COMPONENT REF=<U2>
    (C) PLACING <EINPUT> COMPONENT REF=<IN1>
  (ENDING FUNCTION BLOCK <EINPUT> REF=<IN1>)

  (C) PLACING <EOUTPUT> COMPONENT REF=<OUT1>
(ENDING FUNCTION BLOCK <EOUTPUT> REF=<OUT1>)

Depolarizing EOUTPUT OUT1
Depolarizing EINPUT IN1

| terminal component found by coord (344,128), GND U5 attached to [20/0] |

+---------------------------------------------------------------------------+
|                                                                           |
| S E S S I O N       3                                                     |
|                                                                           |
+---------------------------------------------------------------------------+
Processing node 20 link 0 session 3

-------------------------------------------------------------------
[                F A M I L Y    G R O U P I N G                   ]
-------------------------------------------------------------------
A GND block GND U5 if part of family 1
A component GND U5 if part of family 1
{ surfing node 20 }
A component EOUTPUT OUT2 if part of family 1
  { exploring component EOUTPUT OUT2 }
  { surfing node 16 }
A component EINPUT IN2 if part of family 1
    { exploring component EINPUT IN2 }
    { surfing node 18 }
A component PWR U6 if part of family 1
      { exploring component PWR U6 }
    { exiting due source component PWR U6 }
  { exiting node 16 }
{ exiting node 20 }

-------------------------------------------------------------------------------------------------
[    P H A S E    1    -    E x p l o r i n g    T R E E    ,    a d d    S U M    n o d e s    ]
-------------------------------------------------------------------------------------------------
{ Exploring node 20 which consist of 2 links }
  Plug <B> of Comp <EOUTPUT> REF=<OUT2> Node <20> assigned as OUTPUT
  Plug <A> of Comp <EOUTPUT> REF=<OUT2> Node <16> assigned as INPUT
  (|) Slowly opening door of link 0 in node 20
  (i) Link 0 of node 20 skipped because it is the enter node
  (|) Slowly opening door of link 1 in node 20
  (i) Component EOUTPUT OUT2 is part of the population for node 20
  Surfing inputs for component <EOUTPUT> <OUT2>
  (i) Component EOUTPUT OUT2 has 2 pins
  Invoking ExploreTree for Node 16 coming from the bidirectional a PLUG <A> of COMPONENT <EOUTPUT> REF=<OUT2>
  { Exploring node 16 which consist of 2 links }
    Plug <B> of Comp <EINPUT> REF=<IN2> Node <16> assigned as OUTPUT
    Plug <A> of Comp <EINPUT> REF=<IN2> Node <18> assigned as INPUT
    (|) Slowly opening door of link 0 in node 16
    (i) Component EINPUT IN2 is part of the population for node 16
    Surfing inputs for component <EINPUT> <IN2>
    (i) Component EINPUT IN2 has 2 pins
    Invoking ExploreTree for Node 18 coming from the bidirectional a PLUG <A> of COMPONENT <EINPUT> REF=<IN2>
    { Exploring node 18 which consist of 2 links }
      (|) Slowly opening door of link 0 in node 18
      (i) Link 0 of node 18 skipped because it is the enter node
      (|) Slowly opening door of link 1 in node 18
      (i) Component PWR U6 is part of the population for node 18
      Surfing inputs for component <PWR> <U6>
      (i) Component PWR U6 has 1 pins
      { End exploring node 18 - Tree is POWERED(+) }
      ($) Link 1 of node 18 linked to plug VCC of PWR U6 DOES produce power
    (R) After evaluating node <18> these are the results:
      -> 1 components result to be the population of the forest
      -> 1 link is THE ENTER NODE
      -> 1 links are SOURCED
    { End exploring node 18 - Tree is POWERED(+) }
    Plug B of EINPUT IN2 produces source for the node 16
    (|) Slowly opening door of link 1 in node 16
    (i) Link 1 of node 16 skipped because it is the enter node
    ($) Link 0 of node 16 linked to plug B of EINPUT IN2 DOES produce power
    (x) Link 1 of node 16 linked to plug A of EOUTPUT OUT2 is an input and requires power
  (R) After evaluating node <16> these are the results:
    -> 1 components result to be the population of the forest
    -> 1 link is THE ENTER NODE
    -> 2 links are SOURCED
    -> 1 times a node is marked as one-to-one
  { End exploring node 16 }
  Plug B of EOUTPUT OUT2 produces source for the node 20
  (x) Link 0 of node 20 linked to plug OUT of GND U5 is an input and requires power
  ($) Link 1 of node 20 linked to plug B of EOUTPUT OUT2 DOES produce power
(R) After evaluating node <20> these are the results:
  -> 1 components result to be the population of the forest
  -> 1 link is THE ENTER NODE
  -> 2 links are SOURCED
  -> 1 times a node is marked as one-to-one
{ End exploring node 20 }

------------------------------------------------------------------------------------------
[    P H A S E    2    -    P l a c i n g    R E A D    /    W R I T E    B l o c k s    ]
------------------------------------------------------------------------------------------

------------------------------------------------------------------------
[    P H A S E    3    -    P l a c i n g    C A S T    B L O C K S    ]
------------------------------------------------------------------------

| Terminal component found by session 3 , GND U5 attached to [20/1] |


[---> STARTING TREE [20/0] GND U5 <---] 


-------------------------------------------------------------------
[    P H A S E    4    -    G e n e r a t i n g    P - C o d e    ]
-------------------------------------------------------------------
(STARTING FUNCTION BLOCK <EOUTPUT> REF=<OUT2>)
  (STARTING FUNCTION BLOCK <EINPUT> REF=<IN2>)
    (+) <PWR> POWER COMPONENT REF=<U6>
    (C) PLACING <EINPUT> COMPONENT REF=<IN2>
  (ENDING FUNCTION BLOCK <EINPUT> REF=<IN2>)

  (C) PLACING <EOUTPUT> COMPONENT REF=<OUT2>
(ENDING FUNCTION BLOCK <EOUTPUT> REF=<OUT2>)

Depolarizing EOUTPUT OUT2
Depolarizing EINPUT IN2

| terminal component found by coord (344,176), GND U4 attached to [6/1] |

+---------------------------------------------------------------------------+
|                                                                           |
| S E S S I O N       4                                                     |
|                                                                           |
+---------------------------------------------------------------------------+
Processing node 6 link 1 session 4

-------------------------------------------------------------------
[                F A M I L Y    G R O U P I N G                   ]
-------------------------------------------------------------------
A GND block GND U4 if part of family 1
A component GND U4 if part of family 1
{ surfing node 6 }
A component EOUTPUT OUT3 if part of family 1
  { exploring component EOUTPUT OUT3 }
  { surfing node 13 }
A component EINPUT IN3 if part of family 1
    { exploring component EINPUT IN3 }
    { surfing node 11 }
A component PWR U3 if part of family 1
      { exploring component PWR U3 }
    { exiting due source component PWR U3 }
  { exiting node 13 }
{ exiting node 6 }

-------------------------------------------------------------------------------------------------
[    P H A S E    1    -    E x p l o r i n g    T R E E    ,    a d d    S U M    n o d e s    ]
-------------------------------------------------------------------------------------------------
{ Exploring node 6 which consist of 2 links }
  Plug <B> of Comp <EOUTPUT> REF=<OUT3> Node <6> assigned as OUTPUT
  Plug <A> of Comp <EOUTPUT> REF=<OUT3> Node <13> assigned as INPUT
  (|) Slowly opening door of link 0 in node 6
  (i) Component EOUTPUT OUT3 is part of the population for node 6
  Surfing inputs for component <EOUTPUT> <OUT3>
  (i) Component EOUTPUT OUT3 has 2 pins
  Invoking ExploreTree for Node 13 coming from the bidirectional a PLUG <A> of COMPONENT <EOUTPUT> REF=<OUT3>
  { Exploring node 13 which consist of 2 links }
    Plug <B> of Comp <EINPUT> REF=<IN3> Node <13> assigned as OUTPUT
    Plug <A> of Comp <EINPUT> REF=<IN3> Node <11> assigned as INPUT
    (|) Slowly opening door of link 0 in node 13
    (i) Link 0 of node 13 skipped because it is the enter node
    (|) Slowly opening door of link 1 in node 13
    (i) Component EINPUT IN3 is part of the population for node 13
    Surfing inputs for component <EINPUT> <IN3>
    (i) Component EINPUT IN3 has 2 pins
    Invoking ExploreTree for Node 11 coming from the bidirectional a PLUG <A> of COMPONENT <EINPUT> REF=<IN3>
    { Exploring node 11 which consist of 2 links }
      (|) Slowly opening door of link 0 in node 11
      (i) Component PWR U3 is part of the population for node 11
      Surfing inputs for component <PWR> <U3>
      (i) Component PWR U3 has 1 pins
      { End exploring node 11 - Tree is POWERED(+) }
      ($) Link 0 of node 11 linked to plug VCC of PWR U3 DOES produce power
    (R) After evaluating node <11> these are the results:
      -> 1 components result to be the population of the forest
      -> 1 links are SOURCED
    { End exploring node 11 - Tree is POWERED(+) }
    Plug B of EINPUT IN3 produces source for the node 13
    (x) Link 0 of node 13 linked to plug A of EOUTPUT OUT3 is an input and requires power
    ($) Link 1 of node 13 linked to plug B of EINPUT IN3 DOES produce power
  (R) After evaluating node <13> these are the results:
    -> 1 components result to be the population of the forest
    -> 1 link is THE ENTER NODE
    -> 2 links are SOURCED
    -> 1 times a node is marked as one-to-one
  { End exploring node 13 }
  Plug B of EOUTPUT OUT3 produces source for the node 6
  (|) Slowly opening door of link 1 in node 6
  (i) Link 1 of node 6 skipped because it is the enter node
  ($) Link 0 of node 6 linked to plug B of EOUTPUT OUT3 DOES produce power
  (x) Link 1 of node 6 linked to plug OUT of GND U4 is an input and requires power
(R) After evaluating node <6> these are the results:
  -> 1 components result to be the population of the forest
  -> 1 link is THE ENTER NODE
  -> 2 links are SOURCED
  -> 1 times a node is marked as one-to-one
{ End exploring node 6 }

------------------------------------------------------------------------------------------
[    P H A S E    2    -    P l a c i n g    R E A D    /    W R I T E    B l o c k s    ]
------------------------------------------------------------------------------------------

------------------------------------------------------------------------
[    P H A S E    3    -    P l a c i n g    C A S T    B L O C K S    ]
------------------------------------------------------------------------

| Terminal component found by session 4 , GND U4 attached to [6/1] |


[---> STARTING TREE [6/1] GND U4 <---] 


-------------------------------------------------------------------
[    P H A S E    4    -    G e n e r a t i n g    P - C o d e    ]
-------------------------------------------------------------------
(STARTING FUNCTION BLOCK <EOUTPUT> REF=<OUT3>)
  (STARTING FUNCTION BLOCK <EINPUT> REF=<IN3>)
    (+) <PWR> POWER COMPONENT REF=<U3>
    (C) PLACING <EINPUT> COMPONENT REF=<IN3>
  (ENDING FUNCTION BLOCK <EINPUT> REF=<IN3>)

  (C) PLACING <EOUTPUT> COMPONENT REF=<OUT3>
(ENDING FUNCTION BLOCK <EOUTPUT> REF=<OUT3>)

Depolarizing EOUTPUT OUT3
Depolarizing EINPUT IN3

| terminal component found by coord (344,224), GND U8 attached to [30/0] |

+---------------------------------------------------------------------------+
|                                                                           |
| S E S S I O N       5                                                     |
|                                                                           |
+---------------------------------------------------------------------------+
Processing node 30 link 0 session 5

-------------------------------------------------------------------
[                F A M I L Y    G R O U P I N G                   ]
-------------------------------------------------------------------
A GND block GND U8 if part of family 1
A component GND U8 if part of family 1
{ surfing node 30 }
A component EOUTPUT OUT4 if part of family 1
  { exploring component EOUTPUT OUT4 }
  { surfing node 26 }
A component EINPUT IN4 if part of family 1
    { exploring component EINPUT IN4 }
    { surfing node 28 }
A component PWR U9 if part of family 1
      { exploring component PWR U9 }
    { exiting due source component PWR U9 }
  { exiting node 26 }
{ exiting node 30 }

-------------------------------------------------------------------------------------------------
[    P H A S E    1    -    E x p l o r i n g    T R E E    ,    a d d    S U M    n o d e s    ]
-------------------------------------------------------------------------------------------------
{ Exploring node 30 which consist of 2 links }
  Plug <B> of Comp <EOUTPUT> REF=<OUT4> Node <30> assigned as OUTPUT
  Plug <A> of Comp <EOUTPUT> REF=<OUT4> Node <26> assigned as INPUT
  (|) Slowly opening door of link 0 in node 30
  (i) Link 0 of node 30 skipped because it is the enter node
  (|) Slowly opening door of link 1 in node 30
  (i) Component EOUTPUT OUT4 is part of the population for node 30
  Surfing inputs for component <EOUTPUT> <OUT4>
  (i) Component EOUTPUT OUT4 has 2 pins
  Invoking ExploreTree for Node 26 coming from the bidirectional a PLUG <A> of COMPONENT <EOUTPUT> REF=<OUT4>
  { Exploring node 26 which consist of 2 links }
    Plug <B> of Comp <EINPUT> REF=<IN4> Node <26> assigned as OUTPUT
    Plug <A> of Comp <EINPUT> REF=<IN4> Node <28> assigned as INPUT
    (|) Slowly opening door of link 0 in node 26
    (i) Component EINPUT IN4 is part of the population for node 26
    Surfing inputs for component <EINPUT> <IN4>
    (i) Component EINPUT IN4 has 2 pins
    Invoking ExploreTree for Node 28 coming from the bidirectional a PLUG <A> of COMPONENT <EINPUT> REF=<IN4>
    { Exploring node 28 which consist of 2 links }
      (|) Slowly opening door of link 0 in node 28
      (i) Link 0 of node 28 skipped because it is the enter node
      (|) Slowly opening door of link 1 in node 28
      (i) Component PWR U9 is part of the population for node 28
      Surfing inputs for component <PWR> <U9>
      (i) Component PWR U9 has 1 pins
      { End exploring node 28 - Tree is POWERED(+) }
      ($) Link 1 of node 28 linked to plug VCC of PWR U9 DOES produce power
    (R) After evaluating node <28> these are the results:
      -> 1 components result to be the population of the forest
      -> 1 link is THE ENTER NODE
      -> 1 links are SOURCED
    { End exploring node 28 - Tree is POWERED(+) }
    Plug B of EINPUT IN4 produces source for the node 26
    (|) Slowly opening door of link 1 in node 26
    (i) Link 1 of node 26 skipped because it is the enter node
    ($) Link 0 of node 26 linked to plug B of EINPUT IN4 DOES produce power
    (x) Link 1 of node 26 linked to plug A of EOUTPUT OUT4 is an input and requires power
  (R) After evaluating node <26> these are the results:
    -> 1 components result to be the population of the forest
    -> 1 link is THE ENTER NODE
    -> 2 links are SOURCED
    -> 1 times a node is marked as one-to-one
  { End exploring node 26 }
  Plug B of EOUTPUT OUT4 produces source for the node 30
  (x) Link 0 of node 30 linked to plug OUT of GND U8 is an input and requires power
  ($) Link 1 of node 30 linked to plug B of EOUTPUT OUT4 DOES produce power
(R) After evaluating node <30> these are the results:
  -> 1 components result to be the population of the forest
  -> 1 link is THE ENTER NODE
  -> 2 links are SOURCED
  -> 1 times a node is marked as one-to-one
{ End exploring node 30 }

------------------------------------------------------------------------------------------
[    P H A S E    2    -    P l a c i n g    R E A D    /    W R I T E    B l o c k s    ]
------------------------------------------------------------------------------------------

------------------------------------------------------------------------
[    P H A S E    3    -    P l a c i n g    C A S T    B L O C K S    ]
------------------------------------------------------------------------

| Terminal component found by session 5 , GND U8 attached to [30/0] |


[---> STARTING TREE [30/0] GND U8 <---] 


-------------------------------------------------------------------
[    P H A S E    4    -    G e n e r a t i n g    P - C o d e    ]
-------------------------------------------------------------------
(STARTING FUNCTION BLOCK <EOUTPUT> REF=<OUT4>)
  (STARTING FUNCTION BLOCK <EINPUT> REF=<IN4>)
    (+) <PWR> POWER COMPONENT REF=<U9>
    (C) PLACING <EINPUT> COMPONENT REF=<IN4>
  (ENDING FUNCTION BLOCK <EINPUT> REF=<IN4>)

  (C) PLACING <EOUTPUT> COMPONENT REF=<OUT4>
(ENDING FUNCTION BLOCK <EOUTPUT> REF=<OUT4>)

Depolarizing EOUTPUT OUT4
Depolarizing EINPUT IN4

| terminal component found by coord (344,272), GND U11 attached to [32/1] |

+---------------------------------------------------------------------------+
|                                                                           |
| S E S S I O N       6                                                     |
|                                                                           |
+---------------------------------------------------------------------------+
Processing node 32 link 1 session 6

-------------------------------------------------------------------
[                F A M I L Y    G R O U P I N G                   ]
-------------------------------------------------------------------
A GND block GND U11 if part of family 1
A component GND U11 if part of family 1
{ surfing node 32 }
A component EOUTPUT OUT5 if part of family 1
  { exploring component EOUTPUT OUT5 }
  { surfing node 34 }
A component EINPUT IN5 if part of family 1
    { exploring component EINPUT IN5 }
    { surfing node 33 }
A component PWR U10 if part of family 1
      { exploring component PWR U10 }
    { exiting due source component PWR U10 }
  { exiting node 34 }
{ exiting node 32 }

-------------------------------------------------------------------------------------------------
[    P H A S E    1    -    E x p l o r i n g    T R E E    ,    a d d    S U M    n o d e s    ]
-------------------------------------------------------------------------------------------------
{ Exploring node 32 which consist of 2 links }
  Plug <B> of Comp <EOUTPUT> REF=<OUT5> Node <32> assigned as OUTPUT
  Plug <A> of Comp <EOUTPUT> REF=<OUT5> Node <34> assigned as INPUT
  (|) Slowly opening door of link 0 in node 32
  (i) Component EOUTPUT OUT5 is part of the population for node 32
  Surfing inputs for component <EOUTPUT> <OUT5>
  (i) Component EOUTPUT OUT5 has 2 pins
  Invoking ExploreTree for Node 34 coming from the bidirectional a PLUG <A> of COMPONENT <EOUTPUT> REF=<OUT5>
  { Exploring node 34 which consist of 2 links }
    Plug <B> of Comp <EINPUT> REF=<IN5> Node <34> assigned as OUTPUT
    Plug <A> of Comp <EINPUT> REF=<IN5> Node <33> assigned as INPUT
    (|) Slowly opening door of link 0 in node 34
    (i) Link 0 of node 34 skipped because it is the enter node
    (|) Slowly opening door of link 1 in node 34
    (i) Component EINPUT IN5 is part of the population for node 34
    Surfing inputs for component <EINPUT> <IN5>
    (i) Component EINPUT IN5 has 2 pins
    Invoking ExploreTree for Node 33 coming from the bidirectional a PLUG <A> of COMPONENT <EINPUT> REF=<IN5>
    { Exploring node 33 which consist of 2 links }
      (|) Slowly opening door of link 0 in node 33
      (i) Component PWR U10 is part of the population for node 33
      Surfing inputs for component <PWR> <U10>
      (i) Component PWR U10 has 1 pins
      { End exploring node 33 - Tree is POWERED(+) }
      ($) Link 0 of node 33 linked to plug VCC of PWR U10 DOES produce power
    (R) After evaluating node <33> these are the results:
      -> 1 components result to be the population of the forest
      -> 1 links are SOURCED
    { End exploring node 33 - Tree is POWERED(+) }
    Plug B of EINPUT IN5 produces source for the node 34
    (x) Link 0 of node 34 linked to plug A of EOUTPUT OUT5 is an input and requires power
    ($) Link 1 of node 34 linked to plug B of EINPUT IN5 DOES produce power
  (R) After evaluating node <34> these are the results:
    -> 1 components result to be the population of the forest
    -> 1 link is THE ENTER NODE
    -> 2 links are SOURCED
    -> 1 times a node is marked as one-to-one
  { End exploring node 34 }
  Plug B of EOUTPUT OUT5 produces source for the node 32
  (|) Slowly opening door of link 1 in node 32
  (i) Link 1 of node 32 skipped because it is the enter node
  ($) Link 0 of node 32 linked to plug B of EOUTPUT OUT5 DOES produce power
  (x) Link 1 of node 32 linked to plug OUT of GND U11 is an input and requires power
(R) After evaluating node <32> these are the results:
  -> 1 components result to be the population of the forest
  -> 1 link is THE ENTER NODE
  -> 2 links are SOURCED
  -> 1 times a node is marked as one-to-one
{ End exploring node 32 }

------------------------------------------------------------------------------------------
[    P H A S E    2    -    P l a c i n g    R E A D    /    W R I T E    B l o c k s    ]
------------------------------------------------------------------------------------------

------------------------------------------------------------------------
[    P H A S E    3    -    P l a c i n g    C A S T    B L O C K S    ]
------------------------------------------------------------------------

| Terminal component found by session 6 , GND U11 attached to [32/1] |


[---> STARTING TREE [32/1] GND U11 <---] 


-------------------------------------------------------------------
[    P H A S E    4    -    G e n e r a t i n g    P - C o d e    ]
-------------------------------------------------------------------
(STARTING FUNCTION BLOCK <EOUTPUT> REF=<OUT5>)
  (STARTING FUNCTION BLOCK <EINPUT> REF=<IN5>)
    (+) <PWR> POWER COMPONENT REF=<U10>
    (C) PLACING <EINPUT> COMPONENT REF=<IN5>
  (ENDING FUNCTION BLOCK <EINPUT> REF=<IN5>)

  (C) PLACING <EOUTPUT> COMPONENT REF=<OUT5>
(ENDING FUNCTION BLOCK <EOUTPUT> REF=<OUT5>)

Depolarizing EOUTPUT OUT5
Depolarizing EINPUT IN5
