Processing node 20 link 0 session 3

-------------------------------------------------------------------
[                F A M I L Y    G R O U P I N G                   ]
-------------------------------------------------------------------
A GND block GND U5 if part of family 1
A component GND U5 if part of family 1
{ surfing node 20 }
A component EOUTPUT OUT2 if part of family 1
  { exploring component EOUTPUT OUT2 }
  { surfing node 16 }
A component EINPUT IN2 if part of family 1
    { exploring component EINPUT IN2 }
    { surfing node 18 }
A component PWR U6 if part of family 1
      { exploring component PWR U6 }
    { exiting due source component PWR U6 }
  { exiting node 16 }
{ exiting node 20 }

-------------------------------------------------------------------------------------------------
[    P H A S E    1    -    E x p l o r i n g    T R E E    ,    a d d    S U M    n o d e s    ]
-------------------------------------------------------------------------------------------------
{ Exploring node 20 which consist of 2 links }
  Plug <B> of Comp <EOUTPUT> REF=<OUT2> Node <20> assigned as OUTPUT
  Plug <A> of Comp <EOUTPUT> REF=<OUT2> Node <16> assigned as INPUT
  (|) Slowly opening door of link 0 in node 20
  (i) Link 0 of node 20 skipped because it is the enter node
  (|) Slowly opening door of link 1 in node 20
  (i) Component EOUTPUT OUT2 is part of the population for node 20
  Surfing inputs for component <EOUTPUT> <OUT2>
  (i) Component EOUTPUT OUT2 has 2 pins
  Invoking ExploreTree for Node 16 coming from the bidirectional a PLUG <A> of COMPONENT <EOUTPUT> REF=<OUT2>
  { Exploring node 16 which consist of 2 links }
    Plug <B> of Comp <EINPUT> REF=<IN2> Node <16> assigned as OUTPUT
    Plug <A> of Comp <EINPUT> REF=<IN2> Node <18> assigned as INPUT
    (|) Slowly opening door of link 0 in node 16
    (i) Component EINPUT IN2 is part of the population for node 16
    Surfing inputs for component <EINPUT> <IN2>
    (i) Component EINPUT IN2 has 2 pins
    Invoking ExploreTree for Node 18 coming from the bidirectional a PLUG <A> of COMPONENT <EINPUT> REF=<IN2>
    { Exploring node 18 which consist of 2 links }
      (|) Slowly opening door of link 0 in node 18
      (i) Link 0 of node 18 skipped because it is the enter node
      (|) Slowly opening door of link 1 in node 18
      (i) Component PWR U6 is part of the population for node 18
      Surfing inputs for component <PWR> <U6>
      (i) Component PWR U6 has 1 pins
      { End exploring node 18 - Tree is POWERED(+) }
      ($) Link 1 of node 18 linked to plug VCC of PWR U6 DOES produce power
    (R) After evaluating node <18> these are the results:
      -> 1 components result to be the population of the forest
      -> 1 link is THE ENTER NODE
      -> 1 links are SOURCED
    { End exploring node 18 - Tree is POWERED(+) }
    Plug B of EINPUT IN2 produces source for the node 16
    (|) Slowly opening door of link 1 in node 16
    (i) Link 1 of node 16 skipped because it is the enter node
    ($) Link 0 of node 16 linked to plug B of EINPUT IN2 DOES produce power
    (x) Link 1 of node 16 linked to plug A of EOUTPUT OUT2 is an input and requires power
  (R) After evaluating node <16> these are the results:
    -> 1 components result to be the population of the forest
    -> 1 link is THE ENTER NODE
    -> 2 links are SOURCED
    -> 1 times a node is marked as one-to-one
  { End exploring node 16 }
  Plug B of EOUTPUT OUT2 produces source for the node 20
  (x) Link 0 of node 20 linked to plug OUT of GND U5 is an input and requires power
  ($) Link 1 of node 20 linked to plug B of EOUTPUT OUT2 DOES produce power
(R) After evaluating node <20> these are the results:
  -> 1 components result to be the population of the forest
  -> 1 link is THE ENTER NODE
  -> 2 links are SOURCED
  -> 1 times a node is marked as one-to-one
{ End exploring node 20 }

------------------------------------------------------------------------------------------
[    P H A S E    2    -    P l a c i n g    R E A D    /    W R I T E    B l o c k s    ]
------------------------------------------------------------------------------------------

------------------------------------------------------------------------
[    P H A S E    3    -    P l a c i n g    C A S T    B L O C K S    ]
------------------------------------------------------------------------

| Terminal component found by session 3 , GND U5 attached to [20/1] |


[---> STARTING TREE [20/0] GND U5 <---] 


-------------------------------------------------------------------
[    P H A S E    4    -    G e n e r a t i n g    P - C o d e    ]
-------------------------------------------------------------------
(STARTING FUNCTION BLOCK <EOUTPUT> REF=<OUT2>)
  (STARTING FUNCTION BLOCK <EINPUT> REF=<IN2>)
    (+) <PWR> POWER COMPONENT REF=<U6>
    (C) PLACING <EINPUT> COMPONENT REF=<IN2>
  (ENDING FUNCTION BLOCK <EINPUT> REF=<IN2>)

  (C) PLACING <EOUTPUT> COMPONENT REF=<OUT2>
(ENDING FUNCTION BLOCK <EOUTPUT> REF=<OUT2>)

Depolarizing EOUTPUT OUT2
Depolarizing EINPUT IN2
