Processing node 10 link 1 session 2

-------------------------------------------------------------------
[                F A M I L Y    G R O U P I N G                   ]
-------------------------------------------------------------------
A GND block GND U2 if part of family 1
A component GND U2 if part of family 1
{ surfing node 10 }
A component OUTPUT OUT3 if part of family 1
  { exploring component OUTPUT OUT3 }
  { surfing node 8 }
A component CLOCK CLK1 if part of family 1
    { exploring component CLOCK CLK1 }
  { exiting node 8 }
{ exiting node 10 }

-------------------------------------------------------------------------------------------------
[    P H A S E    1    -    E x p l o r i n g    T R E E    ,    a d d    S U M    n o d e s    ]
-------------------------------------------------------------------------------------------------
{ Exploring node 10 which consist of 2 links }
  Plug <B> of Comp <OUTPUT> REF=<OUT3> Node <10> assigned as OUTPUT
  Plug <A> of Comp <OUTPUT> REF=<OUT3> Node <8> assigned as INPUT
  (|) Slowly opening door of link 0 in node 10
  (i) Component OUTPUT OUT3 is part of the population for node 10
  Surfing inputs for component <OUTPUT> <OUT3>
  (i) Component OUTPUT OUT3 has 2 pins
  Invoking ExploreTree for Node 8 coming from the bidirectional a PLUG <A> of COMPONENT <OUTPUT> REF=<OUT3>
  { Exploring node 8 which consist of 2 links }
    (|) Slowly opening door of link 0 in node 8
    (i) Component CLOCK CLK1 is part of the population for node 8
    Surfing inputs for component <CLOCK> <CLK1>
    (i) State component CLOCK CLK1 was marked as evaluated
    (i) Component CLOCK CLK1 has 1 pins
    (+S+) Assuming link is powered by OUT which is the single output of a state component COMPONENT=<CLOCK> REF=<CLK1>
    (|) Slowly opening door of link 1 in node 8
    (i) Link 1 of node 8 skipped because it is the enter node
    ($) Link 0 of node 8 linked to plug OUT of CLOCK CLK1 DOES produce power
    (x) Link 1 of node 8 linked to plug A of OUTPUT OUT3 is an input and requires power
  (R) After evaluating node <8> these are the results:
    -> 1 components result to be the population of the forest
    -> 1 link is THE ENTER NODE
    -> 2 links are SOURCED
    -> 1 links contains STATE ELEMENTS
    -> 1 times a node is marked as one-to-one
  { End exploring node 8 }
  Plug B of OUTPUT OUT3 produces source for the node 10
  (|) Slowly opening door of link 1 in node 10
  (i) Link 1 of node 10 skipped because it is the enter node
  ($) Link 0 of node 10 linked to plug B of OUTPUT OUT3 DOES produce power
  (x) Link 1 of node 10 linked to plug OUT of GND U2 is an input and requires power
(R) After evaluating node <10> these are the results:
  -> 1 components result to be the population of the forest
  -> 1 link is THE ENTER NODE
  -> 2 links are SOURCED
  -> 1 times a node is marked as one-to-one
{ End exploring node 10 }

------------------------------------------------------------------------------------------
[    P H A S E    2    -    P l a c i n g    R E A D    /    W R I T E    B l o c k s    ]
------------------------------------------------------------------------------------------

------------------------------------------------------------------------
[    P H A S E    3    -    P l a c i n g    C A S T    B L O C K S    ]
------------------------------------------------------------------------

| Terminal component found by session 2 , GND U2 attached to [10/52685] |


[---> STARTING TREE [10/1] GND U2 <---] 


-------------------------------------------------------------------
[    P H A S E    4    -    G e n e r a t i n g    P - C o d e    ]
-------------------------------------------------------------------
(STARTING FUNCTION BLOCK <OUTPUT> REF=<OUT3>)
  (STARTING FUNCTION BLOCK <CLOCK> REF=<CLK1>)
    (C) PLACING <CLOCK> COMPONENT REF=<CLK1>
  (ENDING FUNCTION BLOCK <CLOCK> REF=<CLK1>)

  (M) <CLOCK/OUT> MEMBER CALLING REF=<CLK1>
  (C) PLACING <OUTPUT> COMPONENT REF=<OUT3>
(ENDING FUNCTION BLOCK <OUTPUT> REF=<OUT3>)

Depolarizing OUTPUT OUT3
