Processing node 6 link 0 session 1

-------------------------------------------------------------------
[                F A M I L Y    G R O U P I N G                   ]
-------------------------------------------------------------------
A GND block GND U1 if part of family 1
A component GND U1 if part of family 1
{ surfing node 6 }
A component OUTPUT OUT1 if part of family 1
  { exploring component OUTPUT OUT1 }
  { surfing node 3 }
A component CLOCK CLK1 if part of family 1
    { exploring component CLOCK CLK1 }
  { exiting node 3 }
{ exiting node 6 }

-------------------------------------------------------------------------------------------------
[    P H A S E    1    -    E x p l o r i n g    T R E E    ,    a d d    S U M    n o d e s    ]
-------------------------------------------------------------------------------------------------
{ Exploring node 6 which consist of 2 links }
  Plug <B> of Comp <OUTPUT> REF=<OUT1> Node <6> assigned as OUTPUT
  Plug <A> of Comp <OUTPUT> REF=<OUT1> Node <3> assigned as INPUT
  (|) Slowly opening door of link 0 in node 6
  (i) Link 0 of node 6 skipped because it is the enter node
  (|) Slowly opening door of link 1 in node 6
  (i) Component OUTPUT OUT1 is part of the population for node 6
  Surfing inputs for component <OUTPUT> <OUT1>
  (i) Component OUTPUT OUT1 has 2 pins
  Invoking ExploreTree for Node 3 coming from the bidirectional a PLUG <A> of COMPONENT <OUTPUT> REF=<OUT1>
  { Exploring node 3 which consist of 2 links }
    (|) Slowly opening door of link 0 in node 3
    (i) Component CLOCK CLK1 is part of the population for node 3
    Surfing inputs for component <CLOCK> <CLK1>
    (i) State component CLOCK CLK1 was marked as evaluated
    (i) Component CLOCK CLK1 has 1 pins
    (+S+) Assuming link is powered by OUT which is the single output of a state component COMPONENT=<CLOCK> REF=<CLK1>
    (|) Slowly opening door of link 1 in node 3
    (i) Link 1 of node 3 skipped because it is the enter node
    ($) Link 0 of node 3 linked to plug OUT of CLOCK CLK1 DOES produce power
    (x) Link 1 of node 3 linked to plug A of OUTPUT OUT1 is an input and requires power
  (R) After evaluating node <3> these are the results:
    -> 1 components result to be the population of the forest
    -> 1 link is THE ENTER NODE
    -> 2 links are SOURCED
    -> 1 links contains STATE ELEMENTS
    -> 1 times a node is marked as one-to-one
    -> 1 times a node is marked as directly driven by a single component pin
  { End exploring node 3 }
  Plug B of OUTPUT OUT1 produces source for the node 6
  (x) Link 0 of node 6 linked to plug OUT of GND U1 is an input and requires power
  ($) Link 1 of node 6 linked to plug B of OUTPUT OUT1 DOES produce power
(R) After evaluating node <6> these are the results:
  -> 1 components result to be the population of the forest
  -> 1 link is THE ENTER NODE
  -> 2 links are SOURCED
  -> 1 times a node is marked as one-to-one
  -> 1 times a node is marked as directly driven by a single component pin
{ End exploring node 6 }

------------------------------------------------------------------------------------------
[    P H A S E    2    -    P l a c i n g    R E A D    /    W R I T E    B l o c k s    ]
------------------------------------------------------------------------------------------

------------------------------------------------------------------------
[    P H A S E    3    -    P l a c i n g    C A S T    B L O C K S    ]
------------------------------------------------------------------------

| Terminal component found by session 1 , GND U1 attached to [6/0] |


[---> STARTING TREE [6/0] GND U1 <---] 


-------------------------------------------------------------------
[    P H A S E    4    -    G e n e r a t i n g    P - C o d e    ]
-------------------------------------------------------------------
(STARTING FUNCTION BLOCK <OUTPUT> REF=<OUT1>)
  (STARTING FUNCTION BLOCK <CLOCK> REF=<CLK1>)
    (C) PLACING <CLOCK> COMPONENT REF=<CLK1>
  (ENDING FUNCTION BLOCK <CLOCK> REF=<CLK1>)

  (M) <CLOCK/OUT> MEMBER CALLING REF=<CLK1>
  (C) PLACING <OUTPUT> COMPONENT REF=<OUT1>
(ENDING FUNCTION BLOCK <OUTPUT> REF=<OUT1>)

Depolarizing OUTPUT OUT1
